
# Space separated list of methods to listen for OpenFlow connections from switches
# The default ist "ptcp:" which starts ovs-controller listening on port 6633 on all interfaces.
METHODS="ptcp:"

# Additional options
# OPTIONS=""
