[Dialer defaults]
# Lines begining with # are comments.
# wvdial will look for this file at  /etc/wvdial.conf  or  /home/LoginName/.wvdial.rc

# Redhat/Fedora have an  Internet Connection Wizard in the popup menus
# ICW will write a two part  /etc/wvdial.conf supporting multiple modem usage.

Modem = /home/kolan/.mobile_modem
Baud = 64000
Init1 = ATZ
#Init2 = AT+CGDCONT=1,"IP","internet"
#     ATQ0 V1 E1 S0=0 &C1 &D2 +FCLASS=0
#  Lack of dialtone acquisition can be due to low line voltage,
#    a common problem in Italy.
#  Try inserting a "dial without waiting": X3
#  Init2 = ATQ0 V1 E1 S0=0 X3 &C1 &D2 +FCLASS=0
#  In case of connection instabilities, specify a lower frequency:
#  Init2 = ATQ0 V1 E1 S0=0 X3 &C1 &D2  +MS=34
# ISDN = 0
# Modem Type = Analog Modem
#Phone = *99#
 Phone = *99***1#
# if going through a switch board, a perhaps necessary pause can produced with a comma:
# Phone = 1,Dialout_phone_number
Username = gdata
# if Internet Provider is MSN.net, use under Linux:   MSN/LoginName
Password = gdata

# the following lines is NEEDED only by slmodemd
Carrier check = no
# Kinternet appears to add it automatically.

## If CONNECT is achieved but browsing fails, try activating the following line
 Auto DNS = yes
##    To make a logfile wvdial.out
 wvdial 2>&1 | tee wvdial.out
# #  For some Internet providers, the following line is necessary
 Stupid Mode = yes
##  for other wvdial  options, do "man wvdial" or see the documentation in
##    /usr/share/doc/wvdial/
## End wvdial.conf
